AT A GLANCE

|  |  |
| --- | --- |
| **REGIONAL SIGN** | **STATE SIGN** |
| * High Intensity Vertical Folding Stop Sign * LED Lights (108) * (2) Solar Panels (6V) * Daylight Sensor\* | * High Intensity Vertical Folding Stop Sign * LED Lights (88) * (2) Solar Panels (12V) * Solar Mount * Battery Backup * Bluetooth Connection * Motorized by Arduino * Polycarbonate Casing * Circuit Casing |

\*Change that could have been added to new sign





